**SECTION 08 44 13 – GLAZED ALUMINUM CURTAIN WALLS (VISION 900HP)**

1. GENERAL

 ADMINISTRATIVE REQUIREMENTS

 Pre-Installation Conference:

 Attendance: [Architect,] [Owner,] [Contractor,] [Construction Manager,] [Design/Builder] installer, and related trades.

 Review: Project conditions, manufacturer requirements, delivery and storage, staging and sequencing, and protection of completed work.

 SUBMITTALS

 Action Submittals:

 Shop Drawings: Illustrate products, installation, and relationship to adjacent construction.

 Product Data: Manufacturer’s descriptive data and product attributes.

 Samples:

* + - * 1. [3 x 3] [\_\_ x \_\_] inch [75 x 75] [\_\_ x \_\_] mm coating [selection samples.] [verification samples.].
				2. [12] [\_\_] inch [300] [\_\_] mm long aluminum framing system samples.

 Quality Control Submittals:

 Copy of Miami-Dade Notice of Acceptance.

 Closeout Submittals:

 Maintenance Instructions.

 SYSTEM DESCRIPTION

 Curtain Wall System:

 Tubular aluminum sections with self-supporting framing, factory prefinished, vision glass, [metal panel infill,] and related flashings, anchorage, and attachment devices.

 Pressure-equalized ventilated rainscreen.

 Glazing Method: [Pressure glazed.] [Two-sided structural silicone glazed.] [Four-sided structural silicone glazed.]

 Design Requirements:

* + - 1. Design skylight system to withstand:
				1. Live and dead loads in accordance with Building Code.
				2. Design wind pressure in accordance with [ASCE 7.] [Building Code.] [\_\_\_\_.]
				3. Movement caused by an ambient temperature range of [120] [\_\_] degrees F [49] [\_\_] degrees C and a surface temperature range of [160] [\_\_] degrees F [71] [\_\_] degrees C.
				4. Movement between skylight system and adjacent construction.

 Deflection and Stress Limits:

 Normal to plane of glass, deflection of framing members shall not exceed L/175 or ¾ inch 19 mm, whichever is less. Where joint sealer joint occurs between framing members and building elements, deflection of framing members shall not exceed one half of joint width, or less if required by joint sealer manufacturer.

 In plane of glass, deflection of framing members shall not reduce glass bite below 75 percent of design dimension, and shall not reduce glass edge clearance below 25 percent of design dimension or 1/8 inch 3 mm, whichever is greater. Restrict deflection further if required for assembly and fit of components.

 At connection points of framing members to anchors, anchor deflection in any direction shall not exceed 1/16 inch 1.5 mm.

 Performance Requirements:

 Air infiltration; tested to ASTM E283:

* + - * 1. Maximum 0.00 CFM per square foot 0.01 liters per second at pressure of 1.57 PSF 75 Pa.
				2. Maximum 0.01 CFM per square foot 0.05 liters per second at pressure of 6.27 PSF 300 Pa.
				3. Maximum 0.01 cubic meter per hour per meter, tested to CAN/CSA A440-00 at a pressure difference of 75 Pa, crack length of 10.69 m.

 Water infiltration: No water penetration, tested to ASTM E331 and ASTM E547 at minimum 41.75 PSF 2000 Pa.

 Water infiltration: No water infiltration, tested to CAN/CSA A440-00 at 730 Pa.

 Wind load resistance: Tested to CAN/CSA-A440-00; maximum net deflection measured at mid-height of vertical mullion of 3.35 mm at positive 3330 Pa and 3.26 mm at negative 3330 Pa.

 Structural resistance, tested to ASTM E330:

* + - * 1. Maximum 0.241 inch 6.13 mm deflection at negative 124.89 PSF 5980 Pa.
				2. Maximum 0.278 inch 7.06 mm deflection at positive 124.89 PSF 5980 Pa.
				3. Maximum 0.030 inch 0.76 mm permanent deformation at positive 187.28 PSF 8970 Pa.
				4. Maximum 0.032 inch 0.81 mm permanent deformation at negative 187.28 PSF 8970 Pa.

 QUALITY ASSURANCE

 Installer Qualifications: Minimum [2] [\_\_] years’ experience in work of this Section.

 Mockup: [4 feet 1200 mm wide x 8 feet 2400 mm high.] [\_\_.]

 WARRANTIES

 Manufacturer’s 5 year warranty against air and water infiltration.

 PRODUCTS

 MANUFACTURERS

 Contract Documents are based on Vision 900HP by Unicel Architectural Corp., 800-668-1580, [www.unicelarchitectural.com.](http://www.unicelarchitectural.com.)

 Substitutions: [Under provisions of Division 01.] [Not permitted.]

 MATERIALS

 Aluminum:

 Extrusions: ASTM B221, 6063-T5 alloy and temper.

 Sheet: ASTM B209.

 Steel Shapes: ASTM A36/A36M.

 ACCESSORIES

 Thermal Break Material: Heat-injected Acetal or extruded PVC.

 Flexible Membrane: 0.015 inch 0.4 mm thick.

 Anchors and Fasteners: Stainless or cadmium plated steel.

 Glass and Glazing Accessories: Specified in Section [08 80 00.] [\_\_ \_\_\_\_.]

 Joint Sealers:

 Perimeter: Specified in Section [07 92 00.] [\_\_ \_\_\_\_.]

 Internal: ASTM C920, Type S, Grade NS; single component silicone.

 Rigid Insulation: Minimum R-value of 4.5 per inch RSI value of 0.79 per 25 mm of thickness.

 Primer Paint: Zinc rich type.

 Bituminous Paint.

 FABRICATION

 Accurately fit and secure joints and intersections. Make joints flush, hairline, and weathertight.

 Fabricate in largest practical units.

 Conceal fasteners and attachments from view.

 Drain water occurring within system to exterior.

 Fabricate aluminum components with integral low conductance thermal barrier between exterior and interior exposed components.

 Vent glazing cavity to exterior so that pressure differentials during driving rain conditions will not drive rain past outer glazing cap.

 Reinforce framing members with internal steel when required to support imposed loads.

 Apply bituminous paint to surfaces in contact with dissimilar metals, masonry, or cementitious materials.

 FINISHES

 Aluminum: AA M12C22A31, Class I anodized, clear.

 \*\*\*\* OR \*\*\*\*

 Aluminum: AA M12C22A42, Class I anodized, [[light] [medium] [dark] bronze] [black] [\_\_\_\_] color.

 \*\*\*\* OR \*\*\*\*

 Aluminum:

 Type: AAMA 2603, thermosetting acrylic resin coating.

 Source: Duracron by PPG Industries, Inc. or equivalent.

 Color: [Custom] [\_\_\_\_] color.] [To be selected from manufacturer's full color range.]

\*\*\*\* OR \*\*\*\*

 Aluminum:

 Type: AAMA 2605, fluoropolymer coating containing minimum 70 percent PVDF resins.

 Source: Duranar by PPG Industries, Inc. or equivalent.

 Color: [Custom] [\_\_\_\_] color.] [To be selected from manufacturer's full color range.]

\*\*\*\* OR \*\*\*\*

 Aluminum:

 Type: AAMA 2605, fluoropolymer coating containing minimum 70 percent PVDF resins.

 Source: Duranar Powder Coating by PPG Industries, Inc. or equivalent.

 Color: [Custom] [\_\_\_\_] color.] [To be selected from manufacturer's full color range.]

 Ferrous Metals: [Hot dip galvanized.] [Prime painted.]

 EXECUTION

 INSTALLATION

 Install in accordance with manufacturer's instructions and approved Shop Drawings.

END OF SECTION